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SECTION 09 90 00
PAINTS and COATINGS

MASTER
ARCHITECTURAL PAINTING SPECIFICATION
(Parallel Version – PPG-SW)



The information contained in this Behr Parallel Specification is primarily intended for use in reviewing commercial painting specification submittals. Because coating manufactures may change product formulations, users of this comparative data assume all responsibilities for acceptability of references such as resin types, composition, or gloss levels contained herein. Due to the many variables of Architect’s project painting specifications, it is recommended that the paint manufacturer(s) be contacted for their product’s intended use, technical data, SDS and VOC content compliance with authorities having jurisdiction.
These BEHR PAINTS are in conformance with LEED v4 BUILDING DESIGN AND CONSTRUCTION for LEED v4 BD+C New Construction, Core and Shell, Schools, Retail, Hospitality and Healthcare. All Behr Paints comply with South Coast AQMD Rule 1113. Interior and other Behr Paints are GREENGUARD® Gold Certified.
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1801 E. St. Andrew Place, Santa Ana, California 92705 (714) 545-7101
**  NOTE TO SPECIFIER	This Section is for the specification of coatings in a mild to moderate environment.  It does contain some products from Diamond Vogel’s High Performance product lines to allow for design flexibility.  Diamond Vogel recommends the use of Section 09 96 00 High Performance Coatings for areas that require maximum protection. 
PART 1 - GENERAL
1.01 SUMMARY 
Work includes furnishing of materials and equipment, preparation of surfaces and completion of painting and finishing of surfaces as required by Drawings and specified herein.
1.02 RELATED WORK
A. Factory, pre-finished items as specified in various sections.
B. Shop painting specified in respective sections.
C. Architectural woodworking.
D. Surfaces not to be painted:
1. Pre-finished wall, ceiling and floor coverings.
2. Items with factory-applied final finish.
3. Concealed ducts, pipes and conduit.
4. Surfaces specifically scheduled or noted on Drawings not to be painted. 
1.03 SUBMITTALS
A. Product data:
1. Not less than thirty (30) days before beginning work, submit a complete list of materials proposed for use, together with manufacturer's specifications.
2. Paint materials and products shall be subject to Architect's approval. 
B. Color samples: 
1. Prepare color and finishes on samples, 8-1/2" x 11" in size.
2. Submit samples as requested until required sheen, color and texture is achieved.
3. Prepare wood samples on type and quality of wood specified for use on project.
4. Label and identify each sample as to location and application. 

1.04 COLORS
A. Colors are to be selected or approved by Architect and actual color chips shall be supplied to Contractor for matching. All undercoats shall be tinted to approximately half the color of finish coat.
B. Approval of final colors: Do not apply final coat of paint until colors have been approved by Architect.
C. The number of colors to be used shall be as determined by Architect. Architect reserves right to vary colors throughout project. 
1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver paint materials in sealed original labeled containers bearing manufacturer's name, type of paint, stock number, color and instructions for reducing or mixing where applicable.
B. Paint materials and equipment
1. Store only acceptable project materials on site.
2. Store in a suitable location.
3. Restrict storage to paint materials and related materials.
4. Comply with health and fire regulations.
1.06 PROJECT CONDITIONS
A. Comply with manufacturer's recommendations as to environmental conditions under which coatings and coating systems can be applied. Do not apply paint or coatings when temperature is below 50F. Do not apply exterior paint in damp or rainy weather; ensure that the surface has dried thoroughly before proceeding.  Surface temperature must be at least 5°F above dew point before painting.
B. Do not apply finish in areas where dust or contaminants are being generated.

PART 2 - PRODUCTS
2.01 MATERIALS
A. Basis-of-Design Product: Provide products listed from Behr Paint Company, Santa Ana, California 92705, or comparable products by one of the following. Other manufacturers to conform to materials listed and be approved by Architect.
1. PPG Industries, Inc. (PPG Paints)
2. Sherwin-Williams Company (The)
B. Materials selected for coating systems for each type surface shall be the product of a single manufacturer.
C. Accessory materials such as thinner, linseed oil, putty and shellac shall be of the highest quality and by approved manufacturer, which comply with local VOC content limit regulations.
D. Paints shall be ready-mixed except field catalyzed coatings. 
E. Do not thin finish coats without Architect's approval.
F. Unsuitability of specified products: Claims concerning unsuitability of any material specified or inability to satisfactorily produce the work will not be entertained, unless such claim is made in writing to Architect before work is started.
G. Number of coats scheduled is minimum. Apply additional coats at no additional cost if necessary to completely hide base materials, produce uniform color and provide satisfactory finish result.
H. Submitted paints and coating shall comply with current local, state and federal air quality regulations.
PART 3 - EXECUTION
3.01 EXAMINATION
A. Examine surfaces scheduled to receive paint and finishes for conditions that will adversely affect execution, permanence or quality of work and which cannot be put into acceptable condition through preparatory work as included in Article 3.02 "Preparation ". Notify Owner’s Representative in writing of any defects or conditions which will prevent a satisfactory installation.
B. Examine surfaces scheduled to be finished prior to commencement of work. Report any condition that may potentially effect proper application.
C. Maximum Moisture Content of Substrates: When measured with an electronic moisture meter as follows;
a. Concrete: 12 percent
b. Portland Cement Plaster and Stucco: 12 percent
c. Masonry (Clay and CMU): 12 percent
d. Wood: 15 percent
e. Gypsum Board: 12 percent
D. Portland Cement Plaster Substrates: Verify that plaster is fully cured.
E. Verify suitability of substrates, including surface conditions and compatibility with existing finishes and primers. 
F. Proceed with surface preparation and coating application only after unsatisfactory conditions have been corrected.
1. Application of coating is construed as acceptance of surfaces and conditions. 
3.02 PREPARATION 
A. Clean surfaces to receive paint thoroughly of substances, which could impair adhesion of paints, including dust, dirt, oil and grease before application of any coatings. Prepare surfaces as follows:
1. WOOD SUBSTRATES: Remove mill glaze and dust, sand smooth. Fill open joints, cracks, nail holes and other pits or depressions flush and smooth with wood filler after priming. Use wood putty to match finish paint coat. Touch up knots or sap streaks with a stain-blocking sealer before priming.
2. CONCRETE, PRE-CAST CONCRETE, TILT-UP: Remove release agents, curing compounds, loose particles, efflorescence and chalk.  Do not coat surfaces if moisture content or alkalinity of surface to be coated exceeds that permitted in the manufacturer’s written instructions. Prime with an alkali-resistant primer.
3. PLASTER and STUCCO SUBSTRATES: Fill hairline cracks, small holes and imperfections on surfaces with patching compound. Smooth off to match adjacent surfaces. Apply an alkali-resistant primer or wash with fresh water and neutralize high alkalinity surfaces where they occur. 
4. MASONRY SUBSTRATES: Remove efflorescence and chalk. Do not coat surfaces if moisture content or alkalinity of surface to be coated exceeds that permitted in the manufacturer’s written instructions. Prime with an alkali-resistant primer.
5. SHOP-PRIMED STEEL SUBSTRATES: Solvent clean according to SSPC-SP1. Remove loose primer and rust, contaminants and foreign matter. Prime bare steel and touch up abrasions with a ferrous metal primer.
6. STEEL, FERROUS METAL SUBSTRATES: Remove rust, mill scale, foreign substances and shop primer. Clean according to SSPC-SP3, “Power Tool Cleaning”, or abrasive blasting cleaning according to SSPC-SP6 “Commercial Blast Cleaning” as required. Protect surface from corrosion until application of primer.
7. GALVANIZED METAL: Remove oils, passivators and clean entire surface with an appropriate solvent. Pre-treat with a phosphoric acid etching solution to promote adhesion of subsequently applied coatings.
8. PHOSPHATIZED METAL or GALVANNEALED METAL shall not be chemically etched. Clean and apply suitable metal primer.
9. ALUMINUM SUBSTRATES: Solvent clean according to SSPC-SP1. Remove loose surface oxidation.
10. GYPSUM BOARD SUBSTRATES: Remove dust and foreign matter. Fill pits flush and smooth with joint compound and where required, apply skim coat to provide the required finishing level based on GA-214-96, Recommended Levels of Gypsum Board Finish before application of decoration.
B. Surfaces, which cannot be prepared or painted as specified, shall be immediately brought to attention of Architect in writing.
1. Starting of work without such notification will be considered acceptance by the Contractor of surfaces involved.
2. Replace unsatisfactory work caused by improper or defective surfaces as directed by Architect at no additional cost to Owner. 
3.03 APPLICATION
A. Do not apply initial coating until moisture content of surface is within limitations recommended by paint manufacturer.
B. Application:
1. Apply paint with suitable brushes, rollers or spraying equipment.
2. Apply stain in accordance with manufacturer's recommendations.
3. Rate of application shall not exceed that as recommended by paint manufacturer for surface involved. 
C. Comply with recommendations of product manufacturer for drying time between succeeding coats.
D. Leave parts of molding and ornaments clean and true to details with no undue amount of paint in corners and depressions.
E. Make edges of paint adjoining other material or color clean and sharp with no overlapping.
F. Refinish whole wall where portion of finish is not acceptable.
G. Apply materials evenly with proper film thickness and free of runs, sags, skips and other defects. Hard, glossy finishes shall be sanded lightly between coats, dusted and cleaned before recoating.
H. Remove hardware, hardware accessories, plates, lighting fixtures and similar items in place prior to painting and replaced upon completion of each space.
I. Disconnect heating and other equipment adjacent to walls using workmen skilled in appropriate trades, and moved to permit wall surfaces to be painted. Following completion of painting, they shall be expertly replaced and reconnected.
J. Paint visible surfaces behind vents, registers or grilles flat black.
1. Wash exposed metal with solvent then prime and paint as scheduled.
2. Spray paint wherever practical. 
K. Do not paint over Underwriters' labels, fusible links or sprinkler heads.
L. EXPOSED PLUMBING AND MECHANICAL ITEMS: Items without factory finish such as conduits, pipes, access panels and items of similar nature shall be finished to match adjacent wall and ceiling surfaces unless otherwise directed. 
3.04 CLEANUP
Upon completion of work, remove equipment, excess material and debris, remove paint splatters and leave area in a neat and orderly condition.
3.05 PROTECTION
A. Protect work of other trades, whether to be painted or not, against damage by painting. Correct damage by cleaning, repairing or replacing, and repainting, as acceptable to Architect.
B. Provide "wet paint" signs to protect newly painted finishes. Remove temporary protective wrappings provided by others for protection of their work after completion of painting operations.
1. At completion of construction activities of other trades, touch up and restore damaged or   defaced painted surfaces.
3.06 FINISH SCHEDULE
A. Finish surfaces in accordance with schedule. Catalog names and numbers refer to products as manufactured by the Behr Paint Company, Santa Ana, California 92705, except as otherwise specified. 
B. Provide paint finishes of even uniform color, free from cloudy or mottled appearance. Properly correct non- complying work to satisfaction of Owner’s representative and representative of Behr Process Corporation.

C. Some colors, especially accent colors may require multiple finish coats for adequate coverage and opacity.

D. The specified number of primer and finish coats is minimum acceptable. If full coverage and opacity is not obtained with specified number of coats, apply additional coats as necessary to produce required finish. 

E. Application Finish Schedule:

EXTERIOR PAINT SCHEDULE:


			
	BEHR
	PPG Paints
	Sherwin-Williams



1. Stucco, Cement Plaster
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 

	Topcoat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 



	 Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100

	Topcoat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100



	Semi-Gloss – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Concrete Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Exterior Flat 6-610XI
	A-100 Exterior Flat A6-100 Series

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Exterior Flat 6-610XI
	A-100 Exterior Flat A6-100 Series



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Concrete Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Concrete Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100

	Topcoat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100



2. Stucco and Cement Plaster – High Build Coating
	Flat – Exterior High Build Coating 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Concrete Primer A24W8300

	Intermediate Coat:
	Premium Exterior High Build Coating 4700
	Perma-Crete High Build Acrylic     4-22
	Loxon XP High Build Coating LX11W0051

	Topcoat:
	Premium Exterior High Build Coating 4700
	Perma-Crete High Build Acrylic     4-22
	Loxon XP High Build Coating LX11W0051



3. Stucco, Cement Plaster, Masonry & Brick - Elastomeric
Exterior 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051

	Topcoat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051


	4.	Concrete, Concrete Pre-Cast, Concrete Tilt-Up
	Flat – Exterior, Professional, 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series



	Satin – Exterior, Professional, 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional, Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100


	BEHR
	PPG Paints
	Sherwin-Williams


5. Concrete, Concrete Pre-Cast, Concrete Tilt-Up – High Build Coating
	Flat – Exterior High Build Coating, 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Exterior High Build Coating 4700
	Perma-Crete High Build Acrylic 4-22
	Loxon XP High Build Coating LX11W0051

	Topcoat:
	Premium Exterior High Build Coating 4700
	Perma-Crete High Build Acrylic 4-22
	Loxon XP High Build Coating LX11W0051



6. Concrete, Concrete Pre-Cast, Concrete Tilt-Up – Elastomeric
	Exterior 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051

	Topcoat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051



7. Concrete Masonry Units (CMU)
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series

	Topcoat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series



	Satin – Premium Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100

	Topcoat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100



	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100



Flat – Exterior, Professional 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A6-100 / A-100 Exterior Flat

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A6-100 / A-100 Exterior Flat



	Satin – Exterior, Professional, 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional, Exterior 100% Acrylic 
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	A-100 Latex Gloss A8-100



8. Concrete Masonry Units (CMU) - High Build Coating
	Flat – High Build Coating 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Premium High Build Coating 4700
	Perma-Crete High Build Acrylic 4-22
	Loxon XP High Build Coating LX11W0051

	Topcoat:
	Premium High Build Coating 4700
	Perma-Crete High Build Acrylic 4-22
	Loxon XP High Build Coating LX11W0051



9. Concrete Masonry Units (CMU) - Elastomeric
Exterior 100% Acrylic Elastomeric Coating, 
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W2524

	Intermediate Coat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051

	Topcoat:
	Premium Exterior Elastomeric Paint 68
	Pitt-Flex Elastomeric 4-110 P-C
	Conflex SherLastic CF16W0051




	BEHR
	PPG Paints
	Sherwin-Williams


10. Concrete Porches and Patios
Low Luster Exterior/Interior 100% Acrylic 
	Prime Coat: 
	Concrete Bonding Primer 880*
	None recommended
	Tread-Plex Primer B90W110

	Intermediate Coat:
	Porch/Patio Low Lustre Enamel 6050
	Floor & Porch Satin Latex 3-510
	Porch & Floor Satin A32-200 Series

	Topcoat:
	Porch/Patio Low Lustre Enamel 6050
	Floor & Porch Satin Latex 3-510
	Porch & Floor Satin A32-200 Series


*Note: Intended for use on rough and porous concrete surfaces.

Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880*
	N/A
	N/A

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6705
	N/A
	N/A

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6705
	N/A
	N/A



Note* Intended for use on rough and porous concrete surfaces.

11. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Solid Color Coating
Flat – Premium Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat: 
	Behr Premium DeckOver 5000
	N/A
	SuperDeck Deck & Dock SD9W00151

	Topcoat:
	Behr Premium DeckOver 5000
	N/A 
	SuperDeck Deck & Dock SD9W00151



12. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Textured Solid Color Coating
Flat – Premium Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A
	N/A

	Topcoat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A 
	N/A



13. Wood, Paint Finish
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series

	Topcoat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series



	Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100

	Topcoat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100


	
	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100



	Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85



Flat – Exterior, Professional 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series



	Satin – Exterior, Professional, 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional, Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	17-921 Seal Grip Primer & Sealer
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series




	BEHR
	PPG Paints
	Sherwin-Williams



14. Wood, Paint Finish – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Seal Grip Primer & Sealer 17-921
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss  6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss  6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Seal Grip Primer & Sealer 17-921
	PrepRite ProBlock B51-600

	Intermediate Coat:
	Alkyd Int/Ext Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Alkyd Int/Ext Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Semi-Gloss B53-1250


15. Wood, Stain Finish, Water-Based, Semi-Transparent
	Flat – 100% Acrylic
	Two Coats:
	Semi-Transparent Stain, Sealer 5077
	Sun Proof Ext. S/T Stain 77-1460
	 A15T WoodScapes S/T Stain

	Or - Two Coats:
	Redwood S/T Stain 5330
	
	

	Or – Two Coats
	Cedar Naturaltone S/T Stain 5533
	
	


	
16. Wood, Stain Finish, Water-Based, Solid Color
	Flat – 100% Acrylic
	Two Coats:
	Solid Color Stain White 5011
	Sun Proof Solid Color 77-1310
	Acrystain CK6688 Series

	Or - Two Coats:
	Solid Color Deep Base 5013                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 
	
	

	Or – Two Coats
	Cedar Naturaltone S/T Stain 50533
	
	



17. Wood, Wood Composite – Decks, Patios, Boat Docks, Railings – Solid Color Coating
	Flat – 100% Acrylic, Solid Color Coating
	Two Coats:
	DeckOver Solid Color Coating 5000
	N/A
	SuperDeck Deck & Dock SD9W00151



18. Wood, Wood Composite – Decks, Patios, Boat Docks, Railings – Texture Solid Color Coating
	Flat – 100% Acrylic, Solid Color Coating
	Two Coats:
	DeckOver Texture Coating 5005
	N/A
	N/A



19. Steel, Ferrous Metal
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series

	Topcoat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series



	 Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100

	Topcoat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100


	
	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100



	Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85




	BEHR
	         PPG Paints
	          Sherwin-Williams



Flat – Exterior, Professional 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series



	Satin – Exterior, Professional, 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310 

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional, Exterior 100% Acrylic 
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer        B66-1310

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series



20. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer        B66-1310

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss  6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150


	
	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Seal Grip Primer & Sealer 17-921
	ProCryl Universal Primer        B66-1310

	Intermediate Coat:
	Alkyd Int/Ext Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Alkyd Int/Ext Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250



21. Steel, Ferrous Metal – High Performance, Water-Based, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151

	Topcoat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151



	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051

	Topcoat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051




22. Galvanized Metal, Aluminum, and Non-Ferrous Metals
	Flat – Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series

	Topcoat:
	Premium Plus Exterior Flat 4050
	Manor Hall Exterior Flat 70-101
	SuperPaint Flat A80-1100 Series



	
	
	                  BEHR
	        PPG Paints
	          Sherwin-Williams



	Eggshell (Satin) – Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100

	Topcoat:
	Premium Plus Exterior Satin 9050
	Sun Proof Satin Latex 76-45
	SuperPaint Ext. Satin A89-1100


	
	Semi-Gloss – Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050 
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	Sun Proof Semi-Gloss Latex 78-45
	SuperPaint Ext. Gloss A84-1100



	Gloss – Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Int/Ext  Gloss 52-110
	SuperPaint Ext. High Gloss A85


		Flat – Professional Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Speedhide Acrylic Flat 6-610XI
	A-100 Exterior Flat A6-100 Series



	Satin – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	Speedhide Ext. Satin 6-2045XI
	A-100 Exterior Satin A82-100 



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Speedhide Ext. Semi-Gloss 6-900XI
	Solo Semi-Gloss 76 Series



23. Galvanized Metal, Aluminum, and Non-Ferrous Metals – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150




	Satin – Interior / Exterior Enamel
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250



			BEHR
	       PPG Paints
	     Sherwin-Williams



24. Galvanized Metal, Aluminum, Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer B66W1310

	Intermediate Coat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 

	Topcoat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 


25. Galvanized Metal, Aluminum, Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch GKPA30220
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Pro-Cryl Universal Primer           B66-W01310

	Intermediate Coat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051 

	Topcoat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051 



INTERIOR PAINT SCHEDULE

1. Gypsum Board
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Harmony Primer B11W01500

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance Flat 9-100
	Harmony Flat B05-1000



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Harmony Primer B11W01500

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 9-300XI
	Harmony Eg-Shel B09-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 9-300XI
	Harmony Eg-Shel B09-1000


Satin – Premium Interior, Acrylic
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100


Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Harmony Primer B11W01500

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss      9-500
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss     9-500
	Harmony  Semi-Gloss B10-1000



Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series


Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	Speedhide Zero Interior Latex Sealer        6-4900XI
	ProMar 200 Zero VOC Primer B28W02600 

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat     B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat      B30-2600




			BEHR
	       PPG Paints
	     Sherwin-Williams



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	Speedhide Zero Interior Latex Sealer        6-4900XI
	ProMar 200 Zero VOC Primer B28W02600 

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC      Eg-Shel B20W2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC      Eg-Shel B20W2600



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	Speedhide Zero Interior Latex Sealer        6-4900XI
	ProMar 200 Zero VOC Primer B28W02600 

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar Zero VOC         Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar Zero VOC         Semi-Gloss B31-2600



2. Gypsum Board: Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell




Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss



3. Gypsum Board – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide Water-Borne Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W8111

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250


4. Gypsum Board - Ceilings
Flat – Interior, Acrylic
	Prime Coat:
	Kilz Pro PVA Drywall Primer 10
	Speedhide Latex Sealer 6-2
	PVA Primer Sealer B28W8000

	Intermediate Coat:
	Interior Ceiling Flat 5558
	Ceiling Paint Flat Latex 17-45
	Eminence Ceiling Flat A27

	Topcoat:
	Interior Ceiling Flat 5558
	Ceiling Paint Flat Latex 17-45
	Eminence Ceiling Flat A27


	

			BEHR
	     PPG Paints
	       Sherwin-Williams



5. Gypsum Board - Dry Fall Coating (Spray Applied)
Flat – Interior, Acrylic, Spray Applied
	Prime Coat:
	Kilz Pro PVA Drywall Primer 10
	Speedhide Latex Sealer 6-2
	PVA Primer Sealer B28W8000

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White, 891 Black 
	Speedhide Dry-Fog Flat 6-275Xl 
	Dry Fall Flat B42 Series

	Topcoat:
	Behr Pro Dryfall Flat 890 White, 891 Black 
	Speedhide Dry-Fog Flat 6-275Xl
	Dry Fall Flat B42 Series



6. Concrete, Plaster, Masonry
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell                                                                                                                           9-300Xl
	Harmony Eg-Shel B09-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 9-300Xl
	Harmony Eg-Shel B09-1000



Satin – Premium Interior, Acrylic
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100



	
	Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss 
9-500Xl
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance  Semi-Gloss 
9-500Xl
	Harmony  Semi-Gloss B10-1000


Gloss – Premium Interior, Acrylic
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series



Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat      B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat      B30-2600



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell               6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell               6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC          Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC           Semi-Gloss B31-2600


	





			BEHR
	         PPG Paints
	      Sherwin-Williams



7. Concrete, Plaster, Masonry: Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell



Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Pure Performance Primer 9-900
	Loxon Primer A24W8300

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss


8. Concrete, Plaster, Masonry – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150


9. Concrete, Plaster, Masonry – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Satin – Interior / Exterior Enamel
	Prime Coat:
	All-In-One Primer Sealer 75
	Perma-Crete Primer 4-603
	Loxon Primer A24W8300

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250



10. Concrete Porches and Patios
Low Luster Exterior/Interior 100% Acrylic 
	Prime Coat:
	880 Concrete Bonding Primer*
	N/A
	Tread-Plex Primer B90W110

	Intermediate Coat:
	Premium Porch/Patio Enamel 6050
	Floor & Porch Satin Latex 3-510
	Porch & Floor Satin A32-200 Series

	Topcoat:
	Premium Porch/Patio Enamel 6050
	Floor & Porch Satin Latex 3-510
	Porch & Floor Satin A32-200 Series


	
            *Note: Intended for use on rough and porous concrete surfaces.
Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880* 
	Floor & Porch WB Gloss 3-610
	N/A

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6700
	Floor & Porch WB Gloss 3-610
	N/A

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6700
	Floor & Porch WB Gloss 3-610
	N/A



11. Concrete Masonry Units (CMU)
Flat – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50 
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 9-300Xl 
	Harmony Eg-Shel B09-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 9-300Xl
	Harmony Eg-Shel B09-1000






			BEHR
	         PPG Paints
	      Sherwin-Williams


Satin – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100



	Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss    9-500Xl
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss    9-500Xl
	Harmony  Semi-Gloss B10-1000


	Gloss – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 2-8050
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series



Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat      B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat      B30-2600



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell               6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell               6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC          Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC           Semi-Gloss B31-2600


	
12. Concrete Masonry Units (CMU): Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell



	
	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss





			BEHR
	PPG Paints
	         Sherwin-Williams


13. Concrete Masonry Units (CMU) – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Speedhide Block Filler 6-15
	Block Filler B25W25

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1510
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1510
	WB Alkyd Urethane Low Sheen B53-1250



14. Steel, Ferrous Metal
Flat – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000


	
Eggshell – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell         9-300Xl
	Harmony Eg-Shel B09-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell         9-300Xl
	Harmony Eg-Shel B09-1000



Satin – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100



Semi-Gloss – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Eggshell 9-300Xl
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Eggshell 9-300Xl
	Harmony  Semi-Gloss B10-1000


Gloss – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Pure Performance  Semi-Gloss 
9-500Xl
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Pure Performance  Semi-Gloss 
9-500Xl
	Solo Gloss A77 Series


(Note: 2-8050 Hi-Gloss Enamel conforms to VOC limits of South Coast AQMD Rule 1113.)
Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat          6-4110
	ProMar 200 Zero VOC Flat      B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat          6-4110
	ProMar 200 Zero VOC Flat      B30-2600




			BEHR
	PPG Paints
	         Sherwin-Williams


Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600


Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss 6-4510XI
	ProMar 200 Zero VOC           Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss 6-4510XI
	ProMar 200 Zero VOC          Semi-Gloss B31-2600


15. Steel, Ferrous Metal – Light Industrial Coatings
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell


	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss


	
16. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Premium Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150



	Satin – Premium Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Satin           6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1410
	WB Alkyd Urethane Low Sheen B53-1250



17. Ferrous Metal – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 

	Topcoat:
	Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 


			BEHR
	     PPG Paints
	     Sherwin-Williams




	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051 

	Topcoat:
	Direct-To-Metal Gloss 8200
	Pitt-Tech Plus Gloss DTM 
90-1310
	Pro Industrial DTM Gloss B66W01051 



18. Galvanized Metal, Aluminum, and Non-Ferrous Metals
Flat –Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance Flat 9-100
	Harmony Flat B05-1000


	
	Eggshell – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 
9-300Xl
	Harmony Eg-Shel B09-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Pure Performance Eggshell 
9-300Xl
	Harmony Eg-Shel B09-1000



Satin – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100


	
	Semi-Gloss – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss           9-500Xl
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance Semi-Gloss 
9-500Xl
	Harmony  Semi-Gloss B10-1000



	Gloss – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series


(Note: 2-8050 Hi-Gloss Enamel conforms to VOC limits of South Coast AQMD Rule 1113.)

	Flat – Professional, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat          6-4110
	ProMar 200 Zero VOC Flat      B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat          6-4110
	ProMar 200 Zero VOC Flat      B30-2600









	
			BEHR
	     PPG Paints
	     Sherwin-Williams


	
	Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 6-4310XI
	ProMar 200 Zero VOC Eg-Shel B20-2600


	Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310 

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss 6-4510XI
	ProMar 200 Zero VOC           Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss 6-4510XI
	ProMar 200 Zero VOC          Semi-Gloss B31-2600



19.  Galvanized Metal, Aluminum, and Non-Ferrous Metals – Light Industrial Coatings
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Acrylic Metal Primer M04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Acrylic Metal Primer M04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss



20. Galvanized Metal, Aluminum, and Non-Ferrous Metals – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Premium Interior / Exterior Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150



	Satin – Premium Interior / Exterior Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	Speedhide WB Alkyd Satin           6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	Speedhide WB Alkyd Semi-Gloss 6-1410
	WB Alkyd Urethane Low Sheen B53-1250




			BEHR
	           PPG Paints
	            Sherwin-Williams




21. Galvanized Metal, Aluminum,  Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 

	Topcoat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pitt-Tech Plus Semi-Gloss DTM 90-1210
	Pro Industrial DTM Semi-Gloss B66W01151 



	Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	No recommendation
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	ProCryl Universal Primer       B66W01310

	Intermediate Coat:
	Direct-To-Metal Gloss 8200
	90-1310 Pitt-Tech Plus Gloss DTM 
	Pro Industrial DTM Gloss B66W01051 

	Topcoat:
	Direct-To-Metal Gloss 8200
	90-1310 Pitt-Tech Plus Gloss DTM
	Pro Industrial DTM Gloss B66W01051 




22. Galvanized Metal and Non-Ferrous Metals – Dry Fall Coating (Spray applied) 
	Flat, Acrylic, Dry Fall
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pitt-Tech Plus Primer 90-912
	Multi-Purpose Primer B51-450

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White, 891 Black 
	Speedhide Dry-Fog Flat 6-275Xl
	Dry Fall Flat B42 Series

	Topcoat:
	Behr Pro Dryfall Flat 890 White, 891 Black
	Speedhide Dry-Fog Flat 6-275Xl
	Dry Fall Flat B42 Series



23. WOOD – Paint Finish
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Flat 1050
	Pure Performance  Flat 9-100
	Harmony Flat B05-1000



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	9-300XI Pure Performance  Eggshell
	Harmony Flat B05-1000

	Topcoat:
	Premium Plus Interior Eggshell 2050
	9-300XI Pure Performance  Eggshell
	Harmony Flat B05-1000



Satin – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100

	Topcoat:
	Premium Plus Interior Satin 7050
	Manor Hall Satin 82-400
	Super Paint Satin A87-1100



Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance  Semi-Gloss 
9-500Xl
	Harmony  Semi-Gloss B10-1000

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Pure Performance  Semi-Gloss 
9-500Xl
	Harmony  Semi-Gloss B10-1000






			BEHR
	           PPG Paints
	            Sherwin-Williams



Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050*
	Manor Hall Gloss 52-110
	Solo Gloss A77 Series


(Note: 2-8050 Hi-Gloss Enamel conforms to VOC limits of South Coast AQMD Rule 1113.)

Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat     B30-2600

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	Speedhide Zero Interior Flat 6-4110
	ProMar 200 Zero VOC Flat     B30-2600



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 
6-4310XI
	ProMar 200 Zero VOC Eg-Shel     B20-2600

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	Speedhide Zero Interior Eggshell 
6-4310XI
	ProMar 200 Zero VOC Eg-Shel     B20-2600




Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC           Semi-Gloss B31-2600

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	Speedhide Zero Interior Semi-Gloss           6-4510XI
	ProMar 200 Zero VOC          Semi-Gloss B31-2600


	
24. WOOD – Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pitt-Glaze 16-310 WB Eggshell Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pitt-Glaze 16-510 WB Semi-Gloss Pre-Catalyzed Water-Borne Acrylic Epoxy
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss



25. WOOD – Paint Finish – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	Speedhide WB Alkyd Semi-Gloss 6-1510
	WB Alkyd Urethane Semi-Gloss B53-1150


			
	
			BEHR
	           PPG Paints
	            Sherwin-Williams



	Satin – Premium Interior / Exterior Enamel
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	Speedhide WB Alkyd Satin          6-1410
	WB Alkyd Urethane Low Sheen B53-1250



26. WOOD – Paint Finish – Dry Fall Coating (Spray applied) 
	Flat, Acrylic, Dry Fall
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Pure Performance Primer 9-900
	Premium Wall & Wood Primer B28W08111

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White, 891 Black 
	Speedhide Super Tech WB Dry-Fog Flat 6-725
	Dry Fall Flat B42 Series

	Topcoat:
	Behr Pro Dryfall Flat 890 White, 891 Black
	Speedhide Super Tech WB Dry-Fog Flat 6-725
	Dry Fall Flat B42 Series




END OF SECTION 09 90 00
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