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SECTION 09 90 00
PAINTS and COATINGS

MASTER
ARCHITECTURAL PAINTING SPECIFICATION
(Parallel Version – SW-BM)




The information contained in this Behr Parallel Specification is primarily intended for use in reviewing commercial painting specification submittals. Because coating manufactures may change product formulations, users of this comparative data assume all responsibilities for acceptability of references such as resin types, composition, or gloss levels contained herein. Due to the many variables of Architects’ project painting specifications, it is recommended that the paint manufacturer(s) be contacted for their product’s intended use, technical data, (M)SDS and VOC content compliance with authorities having jurisdiction.
These BEHR PAINTS are in conformance with LEED v4 BUILDING DESIGN AND CONSTRUCTION for LEED v4 BD+C New Construction, Core and Shell, Schools, Retail, Hospitality and Healthcare. All Behr Paints comply with South Coast AQMD Rule 1113. Interior and other Behr Paints are GREENGUARD® Gold Certified.
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1801 E. St. Andrew Place, Santa Ana, California 92705 (714) 545-7101

SECTION 09 90 00 PAINTS AND COATINGS
**  NOTE TO SPECIFIER	This Section is for the specification of coatings in a mild to moderate environment.  It does contain some products from Diamond Vogel’s High Performance product lines to allow for design flexibility.  Diamond Vogel recommends the use of Section 09 96 00 High Performance Coatings for areas that require maximum protection. 
PART 1 - GENERAL
1.01 SUMMARY
Work includes furnishing of materials and equipment, preparation of surfaces and completion of painting and finishing of surfaces as required by Drawings and specified herein.
1.02 RELATED WORK
A. Factory, pre-finished items as specified in various sections.
B. Shop painting specified in respective sections.
C. Architectural woodworking.
D. Surfaces not to be painted:
1. Pre-finished wall, ceiling and floor coverings.
2. Items with factory-applied final finish.
3. Concealed ducts, pipes and conduit.
4. Surfaces specifically scheduled or noted on Drawings not to be painted. 
1.03 SUBMITTALS
A. Product data:
1. Not less than thirty (30) days before beginning work, submit a complete list of materials proposed for use, together with manufacturer's specifications.
2. Paint materials and products shall be subject to Architect's approval. 
B. Color samples: 
1. Prepare color and finishes on samples, 8-1/2" x 11" in size.
2. Submit samples as requested until required sheen, color and texture is achieved.
3. Prepare wood samples on type and quality of wood specified for use on project.
4. Label and identify each sample as to location and application. 

1.04 COLORS
A. Colors are to be selected or approved by Architect and actual color chips shall be supplied to Contractor for matching. All undercoats shall be tinted to approximately half the color of finish coat.
B. Approval of final colors: Do not apply final coat of paint until colors have been approved by Architect.
C. The number of colors to be used shall be as determined by Architect. Architect reserves right to vary colors throughout project. 
1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver paint materials in sealed original labeled containers bearing manufacturer's name, type of paint, stock number, color and instructions for reducing or mixing where applicable.
B. Paint materials and equipment
1. Store only acceptable project materials on site.
2. Store in a suitable location.
3. Restrict storage to paint materials and related materials.
4. Comply with health and fire regulations.
1.06 PROJECT CONDITIONS
A. Comply with manufacturer's recommendations as to environmental conditions under which coatings and coating systems can be applied. Do not apply paint or coatings when temperature is below 50F. Do not apply exterior paint in damp or rainy weather; ensure that the surface has dried thoroughly before proceeding.  Surface temperature must be at least 5°F above dew point before painting.
B. Do not apply finish in areas where dust or contaminants are being generated.

PART 2 - PRODUCTS
2.01 MATERIALS
A. Basis-of-Design Product: Provide products listed from Behr Paint Company, Santa Ana, California 92705, or comparable products by one of the following. Other manufacturers to conform to materials listed and be approved by Architect.
1. Sherwin-Williams Company (The)
2. Benjamin Moore & Company
B. Materials selected for coating systems for each type surface shall be the product of a single manufacturer.
C. Accessory materials such as thinner, linseed oil, putty and shellac shall be of the highest quality and by approved manufacturer, which comply with local VOC content limit regulations.
D. Paints shall be ready-mixed except field catalyzed coatings. 
E. Do not thin finish coats without Architect's approval.
F. Unsuitability of specified products: Claims concerning unsuitability of any material specified or inability to satisfactorily produce the work will not be entertained, unless such claim is made in writing to Architect before work is started.
G. Number of coats scheduled is minimum. Apply additional coats at no additional cost if necessary to completely hide base materials, produce uniform color and provide satisfactory finish result.
H. Submitted paints and coating shall comply with current local, state and federal air quality regulations.

PART 3 - EXECUTION
3.01 EXAMINATION
A. Examine surfaces scheduled to receive paint and finishes for conditions that will adversely affect execution, permanence or quality of work and which cannot be put into acceptable condition through preparatory work as included in Article 3.02 "Preparation ". Notify Owner’s Representative in writing of any defects or conditions which will prevent a satisfactory installation.
B. Examine surfaces scheduled to be finished prior to commencement of work. Report any condition that may potentially effect proper application.
C. Maximum Moisture Content of Substrates: When measured with an electronic moisture meter as follows;
a. Concrete: 12 percent
b. Portland Cement Plaster and Stucco: 12 percent
c. Masonry (Clay and CMU): 12 percent
d. Wood: 15 percent
e. Gypsum Board: 12 percent
D. Portland Cement Plaster Substrates: Verify that plaster is fully cured.
E. Verify suitability of substrates, including surface conditions and compatibility with existing finishes and primers. 
F. Proceed with surface preparation and coating application only after unsatisfactory conditions have been corrected.
1. Application of coating is construed as acceptance of surfaces and conditions. 
3.02 PREPARATION 
A. Surfaces to receive paint shall be clean, dry, and dust free before application of any coatings. Prepare surfaces as follows:
1. WOOD SUBSTRATES: Remove mill glaze and dust, sand smooth. Fill open joints, cracks, nail holes and other pits or depressions flush and smooth with wood filler after priming. Use wood putty to match finish paint coat. Touch up knots or sap streaks with a stain-blocking sealer before priming.
2. CONCRETE: Remove bondbreaker and release agent residue, loose particles, efflorescence and encrustations from cured concrete substrates.  Fill depressions and remove fins and projections not inherent in base material. Prime with an alkali-resistant primer.
3. PRIMED FERROUS METAL: Remove contaminants and foreign matter. Touch up abrasions with a suitable ferrous metal primer.
4. UNPRIMED FERROUS METAL: Remove rust, mill scale and foreign matter by wire-brushing, scraping, abrasive blasting or solvent as required to provide a clean, smooth surface.
5. GALVANIZED METAL: Remove oils, passivators and clean entire surface with an appropriate solvent. Pre-treat with a phosphoric acid etching solution.  Apply primer same day as pretreatment is applied.
6. PHOSPHATIZED METAL shall not be chemically etched. Clean and apply suitable metal primer.
7. GYPSUM BOARD: Remove dust and foreign matter. Fill pits flush and smooth with joint compound and where required skim coat to provide the specified level of finish before application of decoration.
8. PLASTER: Fill hairline cracks, small holes and imperfections on plaster surfaces with patching plaster. Smooth off to match adjacent surfaces. Apply an alkali-resistant primer or wash with fresh water and neutralize high alkalinity surfaces where they occur. 
B. Surfaces, which cannot be prepared or painted as specified, shall be immediately brought to attention of Architect in writing.
1. Starting of work without such notification will be considered acceptance by the Contractor of surfaces involved.
2. Replace unsatisfactory work caused by improper or defective surfaces as directed by Architect at no additional cost to Owner. 
3.03 APPLICATION
A. Do not apply initial coating until moisture content of surface is within limitations recommended by paint manufacturer.
B. Application:
1. Apply paint with suitable brushes, rollers or spraying equipment.
2. Apply stain in accordance with manufacturer's recommendations.
3. Rate of application shall not exceed that as recommended by paint manufacturer for surface involved. 
C. Comply with recommendations of product manufacturer for drying time between succeeding coats.
D. Leave parts of molding and ornaments clean and true to details with no undue amount of paint in corners and depressions.
E. Make edges of paint adjoining other material or color clean and sharp with no overlapping.
F. Refinish whole wall where portion of finish is not acceptable.
G. Apply materials evenly with proper film thickness and free of runs, sags, skips and other defects. Hard, glossy finishes shall be sanded lightly between coats, dusted and cleaned before recoating.
H. Remove hardware, hardware accessories, plates, lighting fixtures and similar items in place prior to painting and replaced upon completion of each space.
I. Disconnect heating and other equipment adjacent to walls using workmen skilled in appropriate trades, and moved to permit wall surfaces to be painted. Following completion of painting, they shall be expertly replaced and reconnected.
J. Paint visible surfaces behind vents, registers or grilles flat black.
1. Wash exposed metal with solvent then prime and paint as scheduled.
2. Spray paint wherever practical. 
K. Do not paint over Underwriters' labels, fusible links or sprinkler heads.
L. EXPOSED PLUMBING AND MECHANICAL ITEMS: Items without factory finish such as conduits, pipes, access panels and items of similar nature shall be finished to match adjacent wall and ceiling surfaces unless otherwise directed. 
3.04 CLEANUP
Upon completion of work, remove equipment, excess material and debris, remove paint splatters and leave area in a neat and orderly condition.
3.05 PROTECTION
A. Protect work of other trades, whether to be painted or not, against damage by painting. Correct damage by cleaning, repairing or replacing, and repainting, as acceptable to Architect.
B. Provide "wet paint" signs to protect newly painted finishes. Remove temporary protective wrappings provided by others for protection of their work after completion of painting operations.
1. At completion of construction activities of other trades, touch up and restore damaged or   defaced painted surfaces.
3.06 FINISH SCHEDULE
A. Finish surfaces in accordance with schedule. Catalog names and numbers refer to products as manufactured by the Behr Paint Company, Santa Ana, California 92705, except as otherwise specified. 
B. Provide paint finishes of even uniform color, free from cloudy or mottled appearance. Properly correct non- complying work to satisfaction of Owner’s representative and representative of Behr Process Corporation.

C. Some colors, especially accent colors may require multiple finish coats for adequate coverage and opacity.

D. The specified number of primer and finish coats is minimum acceptable. If full coverage and opacity is not obtained with specified number of coats, apply additional coats as necessary to produce required finish. 

E. Application Finish Schedule:

	EXTERIOR PAINT SCHEDULE:

			
	BEHR
	Sherwin-Williams
	Benjamin Moore



1. Stucco, Cement Plaster
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	Super Paint Flat A80-1100 
	Moorlife Acrylic Flat N105

	Topcoat:
	Premium Plus Exterior Flat 4050
	Super Paint Flat A80-1100 
	Moorlife Acrylic Flat N105



	Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103



	Semi-Gloss – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449



2. Stucco and Cement Plaster – High Build Coating
	Flat – Premium Exterior High Build Coating 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 

	Topcoat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 



3. Stucco, Cement Plaster, Masonry & Brick - Elastomeric
Exterior Premium 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Low Sheen Elastomeric 68
	SherLastic A5-600 
	Super Spec Elastomeric N055 

	Topcoat:
	Premium Low Sheen Elastomeric 68
	SherLastic A5-600 
	Super Spec Elastomeric N055 


	4.	Concrete, Tilt-Up
	Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	Super Paint Flat A80-100 
	Ultra Spec Ext Flat N447 

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	Super Paint Flat A80-100 
	Ultra Spec Ext Flat N447 



	Satin – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	SuperPaint Ext. Satin A89-1100
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	SuperPaint Ext. Satin A89-1100
	Ultra Spec Ext Satin N448



	Semi-Gloss – Professional Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	SuperPaint Ext. Gloss A84-1100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	SuperPaint Ext. Gloss A84-1100
	Ultra Spec Ext Gloss N449



	BEHR
	Sherwin-Williams
	Benjamin Moore


5. Concrete Tilt-Up – High Build Coating
	Flat – Premium High Build Coating 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 

	Topcoat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 



6. Concrete, Tilt-Up – Elastomeric
Exterior Premium 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300 
	Super Spec Masonry Sealer N066 

	Intermediate Coat:
	Premium Low Sheen Elastomeric 68
	Conflex SherLastic CF16W0051
	Super Spec Elastomeric 055 

	Topcoat:
	Premium Low Sheen Elastomeric 68
	Conflex SherLastic CF16W0051
	Super Spec Elastomeric 055 



7. Concrete Masonry Units (CMU)
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105



	Satin – Premium Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103



	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449



8. Concrete Masonry Units (CMU) - High Build Coating
	Flat – Premium High Build Coating 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 

	Topcoat:
	Premium Flat High Build 4700
	Loxon XP High Build Coating LX11W0051
	Super Spec Masonry Coating 056 



9. Concrete Masonry Units (CMU) - Elastomeric
Exterior Premium 100% Acrylic Elastomeric Coating
	Prime Coat:
	Behr Pro Block Filler50
	Block Filler B25W25 
	Super Spec Block Filler 160 

	Intermediate Coat:
	Premium Low Sheen Elastomeric 68
	Conflex SherLastic CF16W0051
	Super Spec Elastomeric N055 

	Topcoat:
	Premium Low Sheen Elastomeric 68
	Conflex SherLastic CF16W0051
	Super Spec Elastomeric N055 







	BEHR
	Sherwin-Williams
	Benjamin Moore


10. Concrete Porches and Patios
Low Luster Premium Exterior/Interior 100% Acrylic 
	Prime Coat:
	Concrete Bonding Primer 880
	Tread-Plex Primer B90W110 
	Latex Floor & Patio N122 

	Intermediate Coat:
	Premium Porch/Patio Enamel 6050
	Porch & Floor A32-100 
	Latex Floor & Patio N122 

	Topcoat:
	Premium Porch/Patio Enamel 6050
	Porch & Floor A32-100 
	Latex Floor & Patio N122 


         Note *Intended for use on rough and porous concrete surfaces.

Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880*
	N/A
	Latex Floor & Patio Gloss 0121

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6705
	N/A
	Latex Floor & Patio Gloss 0121

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6705
	N/A
	Latex Floor & Patio Gloss 0121


Note* Intended for use on rough and porous concrete surfaces.

11. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Solid Color Coating
Flat – Premium Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat:
	5000 Behr Premium DeckOver
	N/A
	N/A

	Topcoat:
	5000 Behr Premium DeckOver
	N/A 
	N/A



12. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Textured Solid Color Coating
Flat – Premium Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A
	N/A

	Topcoat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A 
	N/A



13. Wood, Paint Finish
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600 
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105



	Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103


	
	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096



	Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309 

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309 



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447 



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600  
	Fresh Start Latex Primer N023 

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449





	BEHR
	Sherwin-Williams
	Benjamin Moore


14. Wood, Paint Finish – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Premium Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	N/A

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss 3900
	WB Alkyd urethane Semi-Gloss B53-1150
	N/A

	Topcoat:
	Urethane Alkyd Semi-Gloss 3900 
	WB Alkyd urethane Semi-Gloss B53-1150
	N/A



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Urethane Alkyd Satin  Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin  Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



15. Wood, Stain Finish, Water-Based, Semi-Transparent
	Flat – 100% Acrylic
	Two Coats:
	Semi-Transparent Stain, Sealer 5077
	WoodScapes S/T Stain A15T 
	Arborcoat WB S/T Stain 638 

	Or - Two Coats:
	Redwood S/T Stain 5033
	
	

	Or – Two Coats
	Cedar Naturaltone S/T Stain 5533
	
	


				
16. Wood, Stain Finish, Water-Based, Solid Color
	Flat – 100% Acrylic
	Two Coats:
	5011 Solid Color Stain 
	Acrystain CK6688 Series 
	Arborcoat Solid Color Stain 640 

	Or - Two Coats:
	5013 Solid Color Deep Base
	
	

	Or – Two Coats
	50533 Cedar Naturaltone S/T Stain
	
	



17. Wood, Wood Composite – Decks, Patios, Boat Docks, Railings – Solid Color Coating
	Flat – Premium 100% Acrylic, Solid Color Coating
	Two Coats:
	5000 DeckOver Solid Color Coating
	N/A
	N/A



18. Wood, Wood Composite – Decks, Patios, Boat Docks, Railings – Texture Solid Color Coating
	Flat – 100% Acrylic, Solid Color Coating
	Two Coats:
	DeckOver Texture Coating 5005
	N/A
	N/A



19. Steel, Ferrous Metal
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66-310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105



	Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66-310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103


	
	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66-310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096



	Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66-310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447



	

	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448


	BEHR
	Sherwin-Williams
	Benjamin Moore


	
	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449



20. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Premium Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer        B66-1310
	N/A

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	N/A

	Topcoat:
	Urethane Alkyd Semi-Gloss 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	N/A


	
	Satin – Premium Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer        B66-1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Urethane Alkyd Satin 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Grand Entrance Satin 147



21. Steel, Ferrous Metal – High Performance, Water-Based, Industrial Maintenance 
	Semi-Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Super Spec HP DTM Acrylic Semi-Gloss P29

	Topcoat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Super Spec HP DTM Acrylic Semi-Gloss P29


	
	Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Super Spec HP DTM Acrylic Gloss P28

	Topcoat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Super Spec HP DTM Acrylic Gloss P28



22. Galvanized Metal, Aluminum, and Non-Ferrous Metals
Flat – Premium Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint A80-1100
	Moorlife Acrylic Flat N105


	Satin – Premium Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Moorgard Low Lustre N103


	



	BEHR
	Sherwin-Williams
	Benjamin Moore


Semi-Gloss – Premium Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050 
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Moorglo Soft Gloss N096



Gloss – Premium Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	SuperPaint Ext. High Gloss A85
	Impervex Latex Gloss W309



Flat – Professional Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Primer A24W8300
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Ultra Spec Ext Flat N447


	
	Satin – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Ultra Spec Ext Satin N448



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Ultra Spec Ext Gloss N449



23. Galvanized Metal, Aluminum, and Non-Ferrous Metals – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Premium Interior / Exterior Alkyd (Water-Reducible) Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	N/A

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	N/A

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	N/A

	Topcoat:
	Urethane Alkyd Semi-Gloss 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	N/A



	Satin – Interior / Exterior Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKPA30220)
	Krud Kutter Metal Clean & Etch 
	Krud Kutter Metal Clean & Etch 

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



24. Galvanized Metal, Aluminum, Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic        Semi-Gloss P29

	Topcoat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic        Semi-Gloss P29



	
	BEHR
	Sherwin-Williams
	  Benjamin Moore


	Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKPA 30220)
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Super Spec DTM Acrylic Gloss P28

	Topcoat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	P28 Super Spec DTM Gloss



	INTERIOR PAINT SCHEDULE

1. Gypsum Board
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



Satin – Premium Interior, Acrylic
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309



Flat – Professional Interior, Acrylic
	Prime Coat:
	Kilz PVA Interior Primer P10
	ProMar 200 Zero VOC Primer B28W2600 
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536




Eggshell – Professional Interior, Acrylic
	Prime Coat:
	Kilz PVA Interior Primer P10
	ProMar 200 Zero VOC Primer B28W2600 
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538



Semi-Gloss – Professional Interior, Acrylic
	Prime Coat:
	Kilz PVA Interior Primer P10
	ProMar 200 Zero VOC Primer B28W2600 
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539



2. Gypsum Board: Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



			BEHR
	Sherwin-Williams
	            Benjamin Moore



Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss



3. Gypsum Board – Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	Premium Wall & Wood Primer B28W8111
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793


	
	Satin – Premium Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	Premium Wall & Wood Primer B28W8111
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aura Grand Entrance Satin 147



4. Gypsum Board - Ceilings
Flat – Interior, Acrylic
	Prime Coat:
	Kilz PVA Interior Primer P10
	Premium Wall & Wood Primer B28W8111
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Interior Ceiling Flat 558
	Eminence Ceiling Flat A27
	Waterborne Ceiling Paint 508

	Topcoat:
	Interior Ceiling Flat 558
	Eminence Ceiling Flat A27
	Waterborne Ceiling Paint 508


	
5. Gypsum Board - Dry Fall Coating (Spray Applied)
Flat – Interior, Acrylic, Spray Applied
	Prime Coat:
	Premium Drywall Primer & Sealer 73
	PrepRite Primer B28W200
	Ultra Spec Latex Primer N534

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	Sweep Up Latex Flat 153

	Topcoat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	Sweep Up Latex Flat 153



6. Concrete, Plaster, Masonry
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547



	
	Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



	Satin – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



	Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



			BEHR
	Sherwin-Williams
	Benjamin Moore


Gloss – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309


	
Flat – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536



Eggshell – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538



Semi-Gloss – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539



7. Concrete, Plaster, Masonry: Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	All-In-One Primer Sealer 75
	Loxon Primer A24W8300
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150          Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150          Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 



8. Concrete, Plaster, Masonry – Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Loxon Primer A24W8300 
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793



	Satin – Interior / Exterior Enamel
	Prime Coat:
	All-In-One Primer Sealer 75
	Loxon Primer A24W8300
	Fresh Start Latex Primer N023

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147




9. Concrete Porches and Patios
Low Luster Exterior/Interior 100% Acrylic 
	Prime Coat:
	Concrete Bonding Primer 880
	Tread-Plex Primer B90W110 
	Latex Floor & Patio N122 

	Intermediate Coat:
	Premium Porch/Patio Enamel 6050
	Porch & Floor A32-100 
	Latex Floor & Patio N122 

	Topcoat:
	Premium Porch/Patio Enamel 6050
	Porch & Floor A32-100 
	Latex Floor & Patio N122 


	
Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880* 
	N/A
	Latex Floor & Patio Gloss 0121

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	Latex Floor & Patio Gloss 0121

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	Latex Floor & Patio Gloss 0121


			BEHR
	Sherwin-Williams 
	  Benjamin Moore



10. Concrete Masonry Units (CMU)
Flat – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50 
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547




Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



Satin – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



Semi-Gloss – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100 
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



Gloss – Premium Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309



Flat – Professional Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536



Eggshell – Professional Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538



Semi-Gloss – Professional Interior, Acrylic
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539



11. Concrete Masonry Units (CMU): Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss




			BEHR
	Sherwin-Williams
	  Benjamin Moore


12. Concrete Masonry Units – Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Behr Pro Block Filler 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793



Satin – Interior / Exterior Enamel
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Super Spec Block Filler 160

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



13. Steel, Ferrous Metal
Flat – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547



Eggshell – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



Satin – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



Semi-Gloss – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



Gloss – Premium Interior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309



Flat – Professional Interior, Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Int. Flat 536



Eggshell – Professional Interior, Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538






			BEHR
	Sherwin-Williams
	        Benjamin Moore



Semi-Gloss – Professional Interior, Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539



14. Steel, Ferrous Metal – Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss



15. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793



	Satin – Premium Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



16. Steel, Ferrous Metal – High Performance, Industrial Maintenance 
	Semi-Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic Semi-Gloss P29

	Topcoat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic Semi-Gloss P29



	Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Super Spec DTM Acrylic Gloss P28

	Topcoat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Super Spec DTM Acrylic Gloss P28



			BEHR
	    Sherwin-Williams
	         Benjamin Moore



17. Galvanized Metal, Aluminum, and Non-Ferrous Metals
Flat – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547


	
	Eggshell – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



Satin –Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



Semi-Gloss – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



	Gloss – Premium Interior 100% Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309



Flat – Professional Interior, Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Interior Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat B30-2600
	Ultra Spec 500 Interior Flat 536



Eggshell – Professional Interior, Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538



Semi-Gloss – Professional Interior, Acrylic
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss B31-2600
	Ultra Spec 500 Semi-Gloss 539






			BEHR
	  Sherwin-Williams
	         Benjamin Moore



18. Galvanized Metal, Aluminum and Non-Ferrous Metals  – Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss



19. Galvanized Metal, Aluminum, and Non-Ferrous Metals – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793


	Satin – Premium Interior / Exterior Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



20. Galvanized Metal, Aluminum,  Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310 
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic        Semi-Gloss P29

	Topcoat:
	Premium Direct-To-Metal Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151 
	Super Spec DTM Acrylic        Semi-Gloss P29



	Gloss, Premium 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Cleaner & Etch
	Krud Kutter Metal Cleaner & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Super Spec DTM Acrylic Gloss P28

	Topcoat:
	Premium Direct-To-Metal Hi-Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Super Spec DTM Acrylic Gloss P28





			BEHR
	    Sherwin-Williams
	        Benjamin Moore



21. Galvanized Metal and Non-Ferrous Metals – Dry Fall Coating (Spray applied) 
	Flat, Acrylic Dry Fall
	Prime Coat:
	Premium Multi-Surface Primer 436
	B51-450 Multi-Purpose Primer
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	153 Sweep Up Latex Flat

	Topcoat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	153 Sweep Up Latex Flat



22. WOOD – Paint Finish
Flat – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547

	Topcoat:
	Premium Plus Interior Flat 1050
	Super Paint Flat A86-100 
	Regal Select Flat 547



Eggshell – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Super Paint Satin A87-1100
	Regal Select Eggshell 549



Satin – Premium Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Regal Select Pearl 550



Semi-Gloss – Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Super Paint Semi-Gloss A88-1100
	Regal Select Semi-Gloss 551



Gloss – Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309

	Topcoat:
	Premium Plus Hi-Gloss 2-8050
	Solo Gloss A77 Series 
	Impervex Latex Gloss W309


Flat – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat      B30-2600
	Ultra Spec 500 Interior Flat 536

	Topcoat:
	Behr Pro Interior Dead Flat 310
	ProMar 200 Zero VOC Flat      B30-2600
	Ultra Spec 500 Interior Flat 536


				
Eggshell – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538

	Topcoat:
	Behr Pro Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	Ultra Spec 500 Eggshell 538



Semi-Gloss – Professional Interior, Acrylic
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss   B31-2600
	Ultra Spec 500 Semi-Gloss 539

	Topcoat:
	Behr Pro Interior Semi-Gloss 370
	ProMar Zero VOC Semi-Gloss   B31-2600
	Ultra Spec 500 Semi-Gloss 539


	
			BEHR
	         Sherwin-Williams
	            Benjamin Moore




23. Wood Paint Finish – Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	Corotech V342 Pre-Catalyzed Waterborne Epoxy Eggshell 



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Super Spec Metal Primer P04

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss 

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150   Semi-Gloss
	Corotech V341 Pre-Catalyzed Waterborne Epoxy Semi-Gloss



24. WOOD – Paint Finish – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Premium Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Advance Waterborne Alkyd 793



Satin – Premium Interior / Exterior Enamel
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Fresh Start Primer N023

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aura Grand Entrance Satin 147



25. WOOD – Paint Finish – Dry Fall Coating (Spray applied) 
	Flat, Acrylic Dry Fall
	Prime Coat:
	Premium All-In-One Primer Sealer 75
	Premium Wall & Wood Primer B28W08111
	Ultra Spec Latex Primer N534 

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	Sweep Up Latex Flat 153

	Topcoat:
	Behr Pro Dryfall Flat 890 White 891 Black
	Dry Fall Flat B42 Series
	Sweep Up Latex Flat 153




END OF SECTION 09 90 00

                                                                                                                                                                                                                                 9-20-2019
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