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SECTION 09 90 00 PAINTS and COATINGS

MASTER
ARCHITECTURAL PAINTING SPECIFICATION
(Parallel Version SW-DE)




The information contained in this Behr Parallel Specification is primarily intended for use in reviewing commercial painting specification submittals. Because coating manufactures may change product formulations, users of this comparative data assume all responsibilities for acceptability of references such as resin types, composition, or gloss levels contained herein. Due to the many variables of Architects’ project painting specifications, it is recommended that the paint manufacturer(s) be contacted for their product’s intended use, technical data, SDS and VOC content compliance with authorities having jurisdiction.

These BEHR PAINTS are in conformance with LEED v4 BUILDING DESIGN AND CONSTRUCTION for LEED v4 BD+C New Construction, Core and Shell, Schools, Retail, Hospitality and Healthcare. All Behr Paints comply with South Coast AQMD Rule 1113. Interior and other Behr Paints are GREENGUARD® Gold Certified.
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SECTION 09 90 00 PAINTS AND COATINGS
**  NOTE TO SPECIFIER	This Section is for the specification of coatings in a mild to moderate environment.  It does contain some products from Diamond Vogel’s High Performance product lines to allow for design flexibility.  Diamond Vogel recommends the use of Section 09 96 00 High Performance Coatings for areas that require maximum protection. 
PART 1 - GENERAL
1.01 SUMMARY
Work includes furnishing of materials and equipment, preparation of surfaces and completion of painting and finishing of surfaces as required by Drawings and specified herein.
1.02 RELATED WORK
A. Factory, pre-finished items as specified in various sections.
B. Shop painting specified in respective sections.
C. Architectural woodworking.
D. Surfaces not to be painted:
1. Pre-finished wall, ceiling and floor coverings.
2. Items with factory-applied final finish.
3. Concealed ducts, pipes and conduit.
4. Surfaces specifically scheduled or noted on Drawings not to be painted. 
1.03 SUBMITTALS
A. Product data:
1. Not less than thirty (30) days before beginning work, submit a complete list of materials proposed for use, together with manufacturer's specifications.
2. Paint materials and products shall be subject to Architect's approval. 
B. Color samples: 
1. Prepare color and finishes on samples, 8-1/2" x 11" in size.
2. Submit samples as requested until required sheen, color and texture is achieved.
3. Prepare wood samples on type and quality of wood specified for use on project.
4. Label and identify each sample as to location and application. 

1.04 COLORS
A. Colors are to be selected or approved by Architect and actual color chips shall be supplied to Contractor for matching. All undercoats shall be tinted to approximately half the color of finish coat.
B. Approval of final colors: Do not apply final coat of paint until colors have been approved by Architect.
C. The number of colors to be used shall be as determined by Architect. Architect reserves right to vary colors throughout project. 
1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver paint materials in sealed original labeled containers bearing manufacturer's name, type of paint, stock number, color and instructions for reducing or mixing where applicable.
B. Paint materials and equipment
1. Store only acceptable project materials on site.
2. Store in a suitable location.
3. Restrict storage to paint materials and related materials.
4. Comply with health and fire regulations.

1.06 PROJECT CONDITIONS
A. Comply with manufacturer's recommendations as to environmental conditions under which coatings and coating systems can be applied. Do not apply paint or coatings when temperature is below 50F. Do not apply exterior paint in damp or rainy weather; ensure that the surface has dried thoroughly before proceeding.  Surface temperature must be at least 5°F above dew point before painting.
B. Do not apply finish in areas where dust or contaminants are being generated.

PART 2 - PRODUCTS
2.01 MATERIALS
A. Basis-of-Design Product: Provide products listed from Behr Paint Company, Santa Ana, California 92705, or comparable products by one of the following. Other manufacturers to conform to materials listed and be approved by Architect.
1. Kelly-Moore Paint Company
2. Dunn-Edwards Corporation
B. Materials selected for coating systems for each type surface shall be the product of a single manufacturer.
C. Accessory materials such as thinner, linseed oil, putty and shellac shall be of the highest quality and by approved manufacturer, which comply with local VOC content limits regulations.
D. Paints shall be ready-mixed except field catalyzed coatings. 
E. Do not thin finish coats without Architect's approval.
F. Unsuitability of specified products: Claims concerning unsuitability of any material specified or inability to satisfactorily produce the work will not be entertained, unless such claim is made in writing to Architect before work is started.
G. Number of coats scheduled is minimum. Apply additional coats at no additional cost if necessary to completely hide base materials, produce uniform color and provide satisfactory finish result.
H. Submitted paints and coatings comply with the established VOC content limits of South Coast AQMD Rule 1113.
PART 3 - EXECUTION
3.01 EXAMINATION
A. Examine surfaces scheduled to receive paint and finishes for conditions that will adversely affect execution, permanence or quality of work and which cannot be put into acceptable condition through preparatory work as included in Article 3.02 "Preparation ". Notify Owner’s Representative in writing of any defects or conditions which will prevent a satisfactory installation.
B. Examine surfaces scheduled to be finished prior to commencement of work. Report any condition that may potentially effect proper application.
C. Maximum Moisture Content of Substrates: When measured with an electronic moisture meter as follows;
a. Concrete: 12 percent
b. Portland Cement Plaster and Stucco: 12 percent
c. Masonry (Clay and CMU): 12 percent
d. Wood: 15 percent
e. Gypsum Board: 12 percent
D. Portland Cement Plaster Substrates: Verify that plaster is fully cured.
E. Verify suitability of substrates, including surface conditions and compatibility with existing finishes and primers. 
F. Proceed with surface preparation and coating application only after unsatisfactory conditions have been corrected.
1. Application of coating is construed as acceptance of surfaces and conditions. 
3.02 PREPARATION 
A. Clean surfaces to receive paint thoroughly of substances, which could impair adhesion of paints, including dust, dirt, oil and grease before application of any coatings. Prepare surfaces as follows:
1. WOOD SUBSTRATES: Remove mill glaze and dust, sand smooth. Fill open joints, cracks, nail holes and other pits or depressions flush and smooth with wood filler after priming. Use wood putty to match finish paint coat. Touch up knots or sap streaks with a stain-blocking sealer before priming.
2. CONCRETE, PRE-CAST CONCRETE, TILT-UP: Remove release agents, curing compounds, loose particles, efflorescence and chalk.  Do not coat surfaces if moisture content or alkalinity of surface to be coated exceeds that permitted in the manufacturer’s written instructions. Prime with an alkali-resistant primer.
3. PLASTER and STUCCO SUBSTRATES: Fill hairline cracks, small holes and imperfections on surfaces with patching compound. Smooth off to match adjacent surfaces. Apply an alkali-resistant primer or wash with fresh water and neutralize high alkalinity surfaces where they occur. 
4. MASONRY SUBSTRATES: Remove efflorescence and chalk. Do not coat surfaces if moisture content or alkalinity of surface to be coated exceeds that permitted in the manufacturer’s written instructions. Prime with an alkali-resistant primer.
5. SHOP-PRIMED STEEL SUBSTRATES: Solvent clean according to SSPC-SP1. Remove loose primer and rust, contaminants and foreign matter. Prime bare steel and touch up abrasions with a ferrous metal primer.
6. STEEL, FERROUS METAL SUBSTRATES: Remove rust, mill scale, foreign substances and shop primer. Clean according to SSPC-SP3, “Power Tool Cleaning”, or abrasive blasting cleaning according to SSPC-SP6 “Commercial Blast Cleaning” as required. Protect surface from corrosion until application of primer.
7. GALVANIZED METAL: Remove oils, passivators and clean entire surface with an appropriate solvent. Pre-treat with a phosphoric acid etching solution to promote adhesion of subsequently applied coatings.
8. PHOSPHATIZED METAL or GALVANNEALED METAL shall not be chemically etched. Clean and apply suitable metal primer.
9. ALUMINUM SUBSTRATES: Solvent clean according to SSPC-SP1. Remove loose surface oxidation.
10. GYPSUM BOARD SUBSTRATES: Remove dust and foreign matter. Fill pits flush and smooth with joint compound and where required, apply skim coat to provide the required finishing level based on GA-214-96, Recommended Levels of Gypsum Board Finish before application of decoration.
B. Surfaces, which cannot be prepared or painted as specified, shall be immediately brought to attention of Architect in writing.
1. Starting of work without such notification will be considered acceptance by the Contractor of surfaces involved.
2. Replace unsatisfactory work caused by improper or defective surfaces as directed by Architect at no additional cost to Owner. 
3.03 APPLICATION
A. Do not apply initial coating until moisture content of surface is within limitations recommended by paint manufacturer.
B. Application:
1. Apply paint with suitable brushes, rollers or spraying equipment.
2. Apply stain in accordance with manufacturer's recommendations.
3. Rate of application shall not exceed that as recommended by paint manufacturer for surface involved. 
C. Comply with recommendations of product manufacturer for drying time between succeeding coats.
D. Leave parts of molding and ornaments clean and true to details with no undue amount of paint in corners and depressions.
E. Make edges of paint adjoining other material or color clean and sharp with no overlapping.
F. Refinish whole wall where portion of finish is not acceptable.
G. Apply materials evenly with appropriate film thickness and free of runs, sags, skips and other defects. Hard, glossy finishes shall be sanded lightly between coats, dusted and cleaned before recoating.
H. Remove hardware, hardware accessories, plates, lighting fixtures and similar items in place prior to painting and replaced upon completion of each space.
I. Disconnect heating and other equipment adjacent to walls using workmen skilled in appropriate trades, and moved to permit wall surfaces to be painted. Following completion of painting, they shall be expertly replaced and reconnected.
J. Paint visible surfaces behind vents, registers or grilles flat black.
1. Wash exposed metal with solvent then prime and paint as scheduled.
2. Spray paint wherever practical. 
K. Do not paint over Underwriters' labels, fusible links or sprinkler heads.
L. EXPOSED PLUMBING AND MECHANICAL ITEMS: Items without factory finish such as conduits, pipes, access panels and items of similar nature shall be finished to match adjacent wall and ceiling surfaces unless otherwise directed. 
3.04 CLEANUP
Upon completion of work, remove equipment, excess material and debris, remove paint splatters and leave area in a neat and orderly condition.
3.05 PROTECTION
A. Protect work of other trades, whether to be painted or not, against damage by painting. Correct damage by cleaning, repairing or replacing, and repainting, as acceptable to Architect.
B. Provide "wet paint" signs to protect newly painted finishes. Remove temporary protective wrappings provided by others for protection of their work after completion of painting operations.
1. At completion of construction activities of other trades, touch up and restore damaged or   defaced painted surfaces.
3.06 FINISH SCHEDULE
A. Finish surfaces in accordance with schedule. Catalog names and numbers refer to products as manufactured by the Behr Paint Company, Santa Ana, California 92705, except as otherwise specified. 
B. Provide paint finishes of even uniform color, free from cloudy or mottled appearance. Properly correct non- complying work to satisfaction of Owner’s representative and representative of Behr Process Corporation.

C. Some colors, especially accent colors may require multiple finish coats for adequate coverage and opacity.

D. The specified number of primer and finish coats is minimum acceptable. If full coverage and opacity is not obtained with specified number of coats, apply additional coats as necessary to produce required finish. 

E. Application Finish Schedule:



EXTERIOR PAINT SCHEDULE:


	Behr
	Sherwin-Williams
	Dunn-Edwards



1. Stucco, Cement Plaster
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2



	 Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	ESPR00 Eff-Stop Premium

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2



	Semi-Gloss – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Ext. Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Semi-Gloss EVSH50-2

	Topcoat:
	Premium Plus Ext. Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Semi-Gloss EVSH50-2



Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Ext. Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Ext. Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50



2. Stucco and Cement Plaster – High Build Coating
	Flat – Exterior High Build Waterproof Coating, 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	N/A

	Intermediate Coat:
	Premium High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A

	Topcoat:
	Premium High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A



3. Stucco, Cement Plaster, Masonry and Brick - Elastomeric
Exterior 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Exterior Elastomeric 68 
	Conflex SherLastic CF16W0051
	Enduralastic 10 Elastomeric EDLX10-0

	Topcoat:
	Premium Exterior Elastomeric 68 
	Conflex SherLastic CF16W0051
	Enduralastic 10 Elastomeric EDLX10-0


	4.	Concrete, Tilt-Up
	Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro e600 Ext. Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Ext. Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50





	BEHR
	    Sherwin-Williams
	          Dunn-Edwards



5. Concrete Tilt-Up – High Build Waterproof Coating
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	N/A

	Intermediate Coat:
	Premium Flat High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A

	Topcoat:
	Premium Flat High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A



6. Concrete Tilt-Up – Elastomeric
	Exterior 100% Acrylic Elastomeric Coating
	Prime Coat:
	Premium Multi-Surface Primer 436
	Loxon Concrete Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Exterior Elastomeric 68 
	Conflex Sherlastic Elastomeric CF11W0051
	Enduralastic 10 Elastomeric EDLX10-0

	Topcoat:
	Premium Exterior Elastomeric 68 
	Conflex Sherlastic Elastomeric CF11W0051
	Enduralastic 10 Elastomeric EDLX10-0



7. Concrete Masonry Units (CMU)
	Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH 10-2



	 Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Plus Exterior Satin 9050
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH 40-2

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH 40-2



	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Low Sheen EVSH 40-2

	Topcoat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Low Sheen EVSH 40-2



	Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A6-100 / A-100 Exterior Flat
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A6-100 / A-100 Exterior Flat
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W2524
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	A-100 Latex Gloss A8-100
	Spartashield Semi-Gloss SSHL50



8. Concrete Masonry Units (CMU) - High Build Waterproof Coating
	Flat – High Build Coating 100% Acrylic
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Loxon Concrete Primer A24W8300
	N/A

	Intermediate Coat:
	Premium Flat High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A

	Topcoat:
	Premium Flat High Build Coating 4700
	Loxon XP High Build Coating LX11W0051
	N/A



9. Concrete Masonry Units (CMU) - Elastomeric
Exterior 100% Acrylic Elastomeric Coating
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Exterior Elastomeric 68 
	Conflex SherLastic CF16W0051
	Enduralastic 10 Elastomeric EDLX10-0

	Topcoat:
	Premium Exterior Elastomeric 68 
	Conflex SherLastic CF16W0051
	Enduralastic 10 Elastomeric EDLX10-0














	BEHR
	Sherwin Williams
	Dunn-Edwards




10. Concrete Porches and Patios
Low Luster Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880*
	None recommended
	N/A

	Intermediate Coat:
	Premium Porch/Patio Low Lustre 6050
	Floor & Porch Satin Latex 3-510
	N/A

	Topcoat:
	Premium Porch/Patio Low Lustre 6050
	Floor & Porch Satin Latex 3-510
	N/A



Note* Intended for use on rough porous concrete.

11. Concrete Porches and Patios
Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880*
	N/A
	N/A

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	N/A

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	N/A



Note* Intended for use on rough porous concrete.

12. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Solid Color Coating
Flat – Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat:
	Behr DeckOver Solid Color Coating 5000
	SuperDeck Deck & Dock SD9W00151
	N/A

	Topcoat:
	Behr DeckOver Solid Color Coating 5000
	SuperDeck Deck & Dock SD9W00151
	N/A



13. Concrete, Decks, Walkways, Pool Decks and Sidewalks – Textured Solid Color Coating
Flat – Exterior Solid Color Coating, 100% Acrylic 
	Prime Coat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A
	N/A

	Topcoat:
	Behr Textured DeckOver Solid Color Coating 5005
	N/A 
	N/A



14. Wood, Paint Finish
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2



	Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2


	
	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Semi-Gloss EVSH50-2

	Topcoat:
	Premium Plus Exterior Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield Semi-Gloss EVSH50-2



	Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60


(Note: Behr Premium 2-8050 Hi-Gloss Enamel conforms to VOC limits of South Coast AQMD Rule 1113.)
	Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	E-Z Prime Premium EZPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Exterior Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50


	BEHR
	Sherwin-Williams
	Dunn-Edwards



			
15. Wood, Paint Finish – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	EZ-Prime Premium EZPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristoshield Semi-Gloss ASHL50 

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristoshield Semi-Gloss ASHL50 



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Multi-Surface Primer 436
	PrepRite ProBlock B51-600
	EZ-Prime Premium EZPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Satin       B53-1250
	Aristoshield Eggshell ASHL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Satin       B53-1250
	Aristoshield Eggshell ASHL30



16. Wood, Stain Finish, Water-Based, Semi-Transparent
	Flat – 100% Acrylic
	Two Coats:
	5077 Weatherproofing Semi-Transparent Stain, Sealer
	 WoodScapes S/T Stain A15T
	WPT-3 WeatherPro Stain

	Or - Two Coats:
	5330 Weatherproofing Redwood Semi-Transparent  Stain
	
	

	Or – Two Coats
	5533 Weatherproofing Cedar Naturaltone Semi-Transparent Stain
	
	




17. Wood, Stain Finish, Solid Color
	Flat – 100% Acrylic
	Two Coats:
	5011 Weatherproofing Solid Color Stain  
	WoodScapes Solid Color Stain A15
	Acri-Hues ACHS10

	Or - Two Coats:
	5013 Weatherproofing Solid Color Deep Base
	
	

	Or – Two Coats
	50533 Weatherproofing Cedar Naturaltone           Semi-Transparent  Stain
	
	




18. Wood and Wood Composite – Decks, Patios, Boat Docks, Railings – Solid Color Coating
	Flat – 100% Acrylic, Solid Color Coating
	Two Coats:
	DeckOver Solid Color Coating 5000
	SuperDeck Deck & Dock SD9W00151
	N/A



19. Wood and Wood Composite – Decks, Patios, Boat Docks, Railings – Textured Solid Color Coating
	Flat – 100% Acrylic, Solid Color Coating
	Two Coats:
	Textured DeckOver Solid Color Coating 5005
	N/A
	N/A



20. Steel, Ferrous Metal
Flat – Premium Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2



	 Satin – Premium Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2

	Topcoat:
	Premium Plus Exterior Satin 9050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2



	Semi-Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield SG EVSH 50-2

	Topcoat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield SG EVSH 50-2



	
	BEHR
	Sherwin-Williams
	Dunn-Edwards


Gloss – Premium Exterior 100% Acrylic 
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Hi-Gloss Enamel 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Hi-Gloss Enamel 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60


(Note: Premium Plus 2-8050 Hi-Gloss Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)

	Flat – Professional Exterior 100% Acrylic
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50



21. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible
	Semi-Gloss – Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900
	WB Alkyd Urethane Semi-Gloss     B53-1150
	Aristoshield Semi-Gloss ASHL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss     B53-1150
	Aristoshield Semi-Gloss ASHL50



	Satin – Interior / Exterior Alkyd (Water-Reducible) Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Satin B53-1250
	Aristoshield Eggshell ASHL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Satin B53-1250
	Aristoshield Eggshell ASHL30



22. Steel, Ferrous Metal – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50

	Topcoat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50



24. Steel, Ferrous Metal – High Performance, Industrial Maintenance 
	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60

	Topcoat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60



25. Galvanized Metal, Aluminum, and Non-Ferrous Metals
Flat – Premium Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Flat A80-1100 Series
	Evershield Flat EVSH10-2



	Satin – Premium Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Exterior Flat 4050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2

	Topcoat:
	Premium Plus Exterior Flat 4050
	SuperPaint Ext. Satin A89-1100
	Evershield Low Sheen EVSH40-2


	
	BEHR
	Sherwin-Williams
	Dunn-Edwards



		Semi-Gloss – Premium Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield SG EVSH 50-2

	Topcoat:
	Premium Plus Semi-Gloss 5050
	SuperPaint Ext. Gloss A84-1100
	Evershield SG EVSH 50-2



	Gloss – Premium Exterior 100% Acrylic 
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Hi-Gloss Enamel 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Hi-Gloss Enamel 8050
	SuperPaint Ext. High Gloss A85
	Evershield Gloss EVSH60


(Note: Behr Premium 2-8050 Hi-Gloss Enamel conforms to VOC limits of South Coast AQMD Rule 1113.)

	Flat – Professional Exterior 100% Acrylic
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10

	Topcoat:
	Behr Pro e600 Exterior Flat 610
	A-100 Exterior Flat A6-100 Series
	Spartashield Flat SSHL10



	Satin – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40

	Topcoat:
	Behr Pro e600 Exterior Satin 640
	A-100 Exterior Satin A82-100 
	Spartashield Low Sheen SSHL40



	Semi-Gloss – Professional Exterior 100% Acrylic	
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50

	Topcoat:
	Behr Pro e600 Ext. Semi-Gloss 670
	Solo Semi-Gloss 76 Series
	Spartashield Semi-Gloss SSHL50


26. Galvanized Metal, Aluminum, and Non-Ferrous Metals– Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Alkyd (Water-Reducible) Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristoshield Semi-Gloss ASHL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristoshield Semi-Gloss ASHL50



	Satin – Interior / Exterior Alkyd (Water-Reducible) Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900
	WB Alkyd Urethane Satin B53-1250
	Aristoshield Eggshell ASHL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Satin B53-1250
	Aristoshield Eggshell ASHL30



27. Galvanized Metal, Aluminum, Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50

	Topcoat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50











	BEHR
	Sherwin-Williams
	Dunn-Edwards



28. Galvanized Metal, Aluminum, Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	Pro-Cryl Universal Primer B66W1310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60

	Topcoat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60


INTERIOR PAINT SCHEDULE

1. Gypsum Board
Flat – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Harmony Primer B11W01500
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10



Eggshell – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Harmony Primer B11W01500
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30



Satin – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Premium Wall & Wood Primer B28W8111
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40




Semi-Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Harmony Primer B11W01500
	 Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50



Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Premium Wall & Wood Primer B28W8111
	 Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Ext/Int Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Ext/Int Gloss EVSH60


(Note: Premium Plus Hi-Gloss Enamel 2-8050 conforms to VOC content limits of South Coast AQMD Rule 1113.)

Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	ProMar 200 Zero VOC Primer B28W02600
	 Vinylastic Select VNPR00-1

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat      B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat     B30-2600
	SPARTAZERO Flat SZR010



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	ProMar 200 Zero VOC Primer B28W02600
	 Vinylastic Select VNPR00-1

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20W2600
	SPARTAZERO Eggshell SZR030







	BEHR
	Sherwin-Williams
	Dunn-Edwards


Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Kilz PVA Interior Primer 10
	ProMar 200 Zero VOC Primer B28W02600
	 Vinylastic Select VNPR00-1

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050


	
2. Gypsum Board: Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	N/A

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A



Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	 Vinylastic Select VNPR00-1

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50



3. Gypsum Board – Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Premium Wall & Wood Primer B28W8111
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss  AWLL50


	

	Satin – Interior / Exterior Alkyd Enamel
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	Premium Wall & Wood Primer B28W8111
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aristowall Eggshell AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aristowall Eggshell  AWLL30



4. Gypsum Board - Ceilings
Flat – Latex, Interior
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	PVA Primer Sealer B28W8000
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Premium Plus Interior Ceiling Flat 558
	Eminence Ceiling Flat A27
	Acoustikote W615

	Topcoat:
	Premium Plus Interior Ceiling Flat 558
	Eminence Ceiling Flat A27
	Acoustikote W615


5. Gypsum Board - Dry Fall Coating (Spray Applied)
Flat – Latex, Interior, Spray Applied
	Prime Coat:
	Premium Plus Drywall Primer Sealer 73
	PVA Primer Sealer B28W8000
	Vinylastic Premium VNPR00

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White/891 Black
	Dry Fall Flat B42 Series
	Aquafall Flat W6079

	Topcoat:
	Behr Pro Dryfall Flat 890 White/891 Black
	Dry Fall Flat B42 Series
	Aquafall Flat W6079



6. Concrete, Plaster, Masonry
Flat – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10





	BEHR
	Sherwin-Williams
	Dunn-Edwards



Eggshell – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30



	Satin – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40



Semi-Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50



	Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60


(Note: Premium Plus 2-8050 Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)
	
Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat  B30-2600
	SPARTAZERO Flat SZR010


	
Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050



7. Concrete, Plaster, Masonry: Light Industrial Coating
Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	N/A

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W8111
	 Vinylastic Select VNPR00-1

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50




8. Concrete, Plaster, Masonry – Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900  
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50


	BEHR
	Sherwin-Williams
	Dunn-Edwards



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Loxon Primer A24W8300
	Eff-Stop Premium ESPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen B53-1250
	Aristowall Eggshell AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900  
	WB Alkyd Urethane Low Sheen B53-1250
	Aristowall Eggshell AWLL30



9. Concrete Porches and Patios
	Low Luster Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880* 
	N/A
	N/A

	Intermediate Coat:
	Premium Porch/Patio Low Lustre 6050
	N/A
	N/A

	Topcoat:
	Premium Porch/Patio Low Lustre 6050
	N/A
	N/A


Note* Intended for use on rough porous concrete.

Gloss Exterior/Premium, Latex, Interior, Low Odor/VOC 
	Prime Coat:
	Concrete & Masonry Bonding Primer 880* 
	N/A
	N/A

	Intermediate Coat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	N/A

	Topcoat:
	Premium Porch/Patio Gloss Enamel 6700
	N/A
	N/A



Note* Intended for use on rough porous concrete.

10. Concrete Masonry Units (CMU)
Flat – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10



Eggshell – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30



Satin – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40



Semi-Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50



Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60


(Note: Premium Plus 2-8050 Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)
	
Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat      B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat      B30-2600
	SPARTAZERO Flat SZR010



Eggshell –Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030




	BEHR
	               Sherwin-Williams
	            Dunn-Edwards



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050



	
11. Concrete Masonry Units (CMU) Light Industrial Coating
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	N/A

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eg-Shel
	N/A



	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50



12. Concrete Masonry Units (CMU) – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss    B53-1150
	Aristowall Semi-Gloss AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss       B53-1150
	Aristowall Semi-Gloss AWLL50



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Behr Pro Block Filler Primer 50
	Block Filler B25W25
	Blocfil Premium SBPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen      B53-1250
	Aristowall Eggshell AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen        B53-1250
	Aristowall Eggshell AWLL30



13. Steel, Ferrous Metal
Flat – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10


	
Eggshell – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30



Satin – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40




	Semi-Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50


	
		BEHR
	Sherwin-Williams
	Dunn-Edwards



Gloss – Premium, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60


(Note: Premium Plus 2-8050 Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)

Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat      B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat      B30-2600
	SPARTAZERO Flat SZR010


	
	Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel B20-2600
	SPARTAZERO Eggshell SZR030



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00 2WH

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050


	
14. Ferrous Metal – Light Industrial Coatings
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	ProCryl Universal Primer B66W01310
	N/A

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	N/A

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	N/A


	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50



15. Steel, Ferrous Metal – Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss  AWLL50



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen      B53-1250
	Aristowall Eggshell AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen  B53-1250
	Aristowall Eggshell AWLL30


		BEHR
	                     Sherwin-Williams
	                Dunn-Edwards



16. Steel, Ferrous Metal – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat ENCT60 Semi-Gloss

	Topcoat:
	Direct-To-Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat ENCT50 Semi-Gloss



	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60

	Topcoat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051
	Endura-Coat Gloss ENCT60



17. Galvanized Metal, Aluminum, and Non-Ferrous Metals
Flat – Premium, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10


	
	Eggshell – Premium, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050 
	Harmony Eg-Shel B09-1000
	Everest Eggshell Ever30



Satin – Premium, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40



Semi-Gloss – Premium, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50



	Gloss – Premium, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60

	Topcoat:
	Premium Plus Int/Ext Hi-Gloss 8050
	Solo Gloss A77 Series
	Evershield Gloss EVSH60


(Note: Premium Plus Hi-Gloss 2-8050 Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)

Flat – Professional, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat  B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat  B30-2600
	SPARTAZERO Flat SZR010


	
	
			BEHR
	           PPG Paints
	            Sherwin-Williams



Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel         B20-2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel      B20-2600
	SPARTAZERO Eggshell SZR030



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050



18. Galvanized Metal, Aluminum and Non-Ferrous Metals – Light Industrial Coatings
	Eggshell – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	N/A

	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	ProCryl Universal Primer B66W01310
	N/A

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	N/A

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Eggshell HP140 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K45 -150 Eggshell
	N/A


	Semi-Gloss – Interior Pre-Catalyzed Waterborne Epoxy
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Plus Multi-Surface Primer   436
	ProCryl Universal Primer       B66W01310
	Bloc Rust Premium BRPR00-2WH

	Intermediate Coat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50

	Topcoat:
	Behr Pro Pre-Catalyzed Waterborne Epoxy Semi-Gloss HP150 
	Pro Industrial Pre-Catalyzed Waterbased Epoxy K46 -150 Semi-Gloss
	Enduracat Semi-Gloss Pre-Catalyzed WB Epoxy ENPX50



19. Galvanized Metal, Aluminum, and Non-Ferrous Metals– Urethane Alkyd, Water-Reducible 
	Semi-Gloss – Interior / Exterior Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean  Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss AWLL50



	Satin – Interior / Exterior Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low sheen
B53-1250
	Aristowall Eggshell AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen 
B53-1250
	Aristowall Eggshell AWLL30








		BEHR
	Sherwin-Williams
	Dunn-Edwards



20. Galvanized Metal, Aluminum,  Non-Ferrous Metals – High Performance, Industrial Maintenance 
	Semi-Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean & Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer       B66W01310
	WB Syn-Lustro Primer WSPR00

	Intermediate Coat:
	Direct To Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50

	Topcoat:
	Direct To Metal  Semi-Gloss 3200
	Pro Industrial DTM Semi-Gloss B66W01151
	Endura-Coat Semi-Gloss ENCT50



	Gloss, 100% Acrylic, Direct-To-Metal Enamel
	Pretreatment:
	Klean Strip Prep & Etch (GKA30220)
	Krud Kutter Metal Clean & Etch
	Krud Kutter Metal Clean Etch

	Prime Coat:
	Premium Multi-Surface Primer 436
	ProCryl Universal Primer B66W01310
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Endura-Coat Gloss ENCT60

	Topcoat:
	Direct To Metal Gloss 8200
	Pro Industrial DTM Gloss B66W01051 
	Endura-Coat Gloss ENCT60



21. Galvanized Metal and Non-Ferrous Metals – Dry Fall Coating (Spray applied) 
	Flat, Latex, Dry Fall
	Prime Coat:
	Premium Multi-Surface Primer 436
	Multi-Purpose Primer B51-450
	Ultra-Grip Premium UGPR00

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White/891 Black 
	Dry Fall Flat B42 Series
	Aquafall Flat W6079

	Topcoat:
	Behr Pro Dryfall Flat 890 White/891 Black 
	Dry Fall Flat B42 Series
	Aquafall Flat W6079



22. WOOD – Paint Finish, Opaque
Flat – Premium Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10

	Topcoat:
	Premium Plus Interior Flat 1050
	Harmony Flat B05-1000
	Everest Flat Ever10



Eggshell – Premium Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Premium Plus Interior Eggshell 2050 
	Super Paint Satin A87-1100
	Everest Eggshell Ever30

	Topcoat:
	Premium Plus Interior Eggshell 2050 
	Super Paint Satin A87-1100
	Everest Eggshell Ever30



Satin – Premium Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40

	Topcoat:
	Premium Plus Interior Satin 7050
	Super Paint Satin A87-1100
	Suprema Satin SPMA40



Semi-Gloss – Premium Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50

	Topcoat:
	Premium Plus Interior Semi-Gloss 3050
	Harmony  Semi-Gloss B10-1000
	Everest Semi-Gloss Ever50



Gloss – Premium Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Premium Plus Hi-Gloss Enamel 8050
	Solo Gloss A77 Series
	Evershield Ext/Int Gloss EVSH60-2

	Topcoat:
	Premium Plus Hi-Gloss Enamel 8050
	Solo Gloss A77 Series
	Evershield Ext/Int Gloss EVSH60-2


(Note: Premium Plus 2-8050 Enamel conforms to VOC content limits of South Coast AQMD Rule 1113.)

Flat – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat     B30-2600
	SPARTAZERO Flat SZR010

	Topcoat:
	Behr Pro i300 Interior Flat Paint 310
	ProMar 200 Zero VOC Flat     B30-2600
	SPARTAZERO Flat SZR010


		BEHR
	Sherwin-Williams
	Dunn-Edwards


	
	Eggshell – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel     B20-2600
	SPARTAZERO Eggshell SZR030

	Topcoat:
	Behr Pro i300 Interior Eggshell 330
	ProMar 200 Zero VOC Eg-Shel     B20-2600
	SPARTAZERO Eggshell SZR030



Semi-Gloss – Professional, Latex, Interior, Low Odor/VOC
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050

	Topcoat:
	Behr Pro i300 Interior Semi-Gloss 370
	ProMar 200 Zero VOC           Semi-Gloss B31-2600
	SPARTAZERO Semi-Gloss SZR050




23. WOOD – Paint Finish– Urethane Alkyd, Water-Reducible and Alkyd Waterborne
	Semi-Gloss – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss B53-1150
	Aristowall Semi-Gloss  AWLL50

	Topcoat:
	Urethane Alkyd Semi-Gloss Enamel 3900 
	WB Alkyd Urethane Semi-Gloss   B53-1150
	Aristowall Semi-Gloss  AWLL50



	Satin – Interior / Exterior Enamel
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen    B53-1250
	Aristowall Eggshell  AWLL30

	Topcoat:
	Urethane Alkyd Satin Enamel 7900 
	WB Alkyd Urethane Low Sheen    B53-1250
	Aristowall Eggshell  AWLL30



24. WOOD – Paint Finish – Dry Fall Coating (Spray applied) 
	Flat, Latex, Dry Fall
	Prime Coat:
	Premium Plus All-In-One Primer 75
	Premium Wall & Wood Primer B28W08111
	Inter-Kote Premium IKPR00

	Intermediate Coat:
	Behr Pro Dryfall Flat 890 White/891 Black
	Dry Fall Flat B42 Series
	Aquafall Flat W6079

	Topcoat:
	Behr Pro Dryfall Flat 890 White/891 Black
	Dry Fall Flat B42 Series
	Aquafall Flat W6079
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